Telemetry example

JS1YRU ORIGAMI2 81 7F 87 CC 9B 0B 05 69 89 6C 90 00 00 00 00 9C 9A 36 00 3E 36 E2 5F 4B 42 48 3E 00 


Execution result

Received telemetry bytes: 28 / 28 bytes

Callsign                         : JS1YRU
Satellite Name                   : ORIGAMI2
UVC Enable                       : ENABLE
UVC Level                        : UVC START SUCCESS
Operation Status                 : FINISHED
Current Mode ID                  : NORMAL
Battery Voltage (V)              : 7.94
Battery Current (A)              : 182.83
Battery Temperature (degC)       : 27
SAP y+/y- Surface                : OFF
SAP x- Surface                   : ON
SAP z- Surface                   : OFF
SAP z+ Surface                   : ON
Thin-film Solar Cell             : ON
Switch (CBand Tx)                : OFF
Switch (Extendable Mast)         : OFF
Switch (ADCS)                    : OFF
Switch (Camera)                  : OFF
Switch (Bus Melt)                : OFF
Switch (TFSC_IV)                 : ON
Switch (Unused)                  : OFF
Switch (IMU)                     : ON
Angular Velocity X (deg/s)       : -2.2
Angular Velocity Y (deg/s)       : 1.0
Angular Velocity Z (deg/s)       : -1.9
Last Executed Command ID (OBC)   : 144
OBC Command Execution Result     : 0
Last Executed Command ID (ADCS)  : 0
ADCS Mode                        : START UP
Last Executed Command ID (RasPi) : 0
Bus Transceiver Temp (degC)      : 28
C-band Transmitter Temp (degC)   : 26
OBC Boot Count                   : 54
Reserved Command Count           : 0
Satellite Time (UNIX)            : 1043784287
UVC Normal Threshold (V)         : 7.5
UVC Safe Threshold (V)           : 6.6
UVC Level1 Threshold (V)         : 7.2
UVC Level2 Threshold (V)         : 6.2
Bus Melt Count                   : 0